Line load is calculated based on tributary width: