The design ice thickness ***td*** is be calculated from ASCE7-10 Eq. 10.4-5