In accordance with ASCE7-10 section 10.4.1 ice weight on structural shapes, prismatic members, and other similar shapes ice weight (per linear foot) is calculated as