In accordance with ASCE7-10 Table 4-1 footnote “c”, design loads for trucks and buses must be per AASHTO LRFD Bridge Design Specifications, therefore