Uniformly distributed live load is determined from ASCE7-10 Table 4-1 for occupancy of type ~OccupancyDescription ~OccupancyNotes

Live load reduction is not permitted for this occupancy.