Uniformly distributed live load is determined from ASCE7-10 Table 4-1 for occupancy of type "~OccupancyDescription"

Additionally a partition live load allowance in accordance with ASCE7-10 section 4.3.2 has been assumed

Total live load used for design is