For the “~SystemDescription” seismic lateral system (~SeismicLateralSystemId) the response modification coefficient, , (in accordance with ASCE7-10 Table 12.2-1)is