The seismic response coefficient, ***Cs*** , (for the constant velocity segment) (for ) is determined in accordance with ASCE7-10 (12.8-3) as: