The seismic response coefficient, ***Cs*** , need not exceed the constant acceleration segment value determined in accordance with ASCE7-10 (12.8-2) as: