In accordance with ASCE7-10 section 11.6 for Risk Category ~RiskCategory, since mapped spectral response acceleration parameter at 1-s period,

Seismic Design Category **~CategoryS1** is assigned to the structure.