Short-period site coefficient (at 0.2 s-period) is determined by interpolation of values in Table 11.4-1 for and for Site Class **~SiteClass**: