Ground snow load, ***pg*** for the location having Latitude ~Latitude, and Longitude ~Longitude at the elevation ~Z ft must be determined based on site-specific Case Studies in accordance with ASCE7-10 figure 7-1.