Snow load (for monoslope, hip and gable roofs with slopes ≤15°, and curved roofs where the vertical angle from

the eaves to the crown is ≤10°) cannot be less than minimum snow load, ***pm*** in accordance with ASCE7-10 7.3.4

For ground snow ≤ 20 psf