Based on ground surface roughness of the upwind terrain for the given wind direction Exposure Category **~ExposureCategory** is used.