Gust-effect factor ***G*** for flexible or dynamically sensitive buildings or other structures is calculated as per ASCE7-10 section 26.9.5 Eq. 26.9-10: