Gust-effect factor ***G*** for rigid buildings or other structures is calculated as per ASCE7-10 section 26.9.4 Eq. 26.9-6: