External Pressure Coefficient, ***Cp*** for Main wind force resisting system (MWFRS) enclosed or partially enclosed building for is taken in accordance ASCE7-10 Figure 27.4-1. For side wall surface