For components and cladding (C&C) external pressure coefficient ***GCp*** is calculated from ASCE7-10 Figure 30.4-1. For effective (tributary) area ofcorner zone (Zone 5) external pressure coefficient is:

|  |  |
| --- | --- |
| Positive (pressure) | Negative (suction) |
|  |  |

Note: a 10% reduction for is taken as permitted in Note 5.