For components and cladding (C&C) external pressure coefficient ***GCp*** is calculated from ASCE7-10 Figure 30.4-1. For effective (tributary) area of middle zone (Zone 4) external pressure coefficient is:

|  |  |
| --- | --- |
| Positive (pressure) | Negative (suction) |
|  |  |