For a partially enclosed building containing a single, unpartitioned large volume, the internal pressure coefficient, (***GCpi***), is be multiplied by the reduction factor, ***Ri***  in accordance with ASCE7-10 equation 26.11-1