Enclosure is classified in accordance with ASCE7-10 section 26.2, as **Enclosed** since it does not meet the open building criteria (in which each wall at least 80% open) nor partially enclosed building (which meets both the criteria that 1) the total area of openings in a wall that receives positive external pressure exceeds the sum of the areas of openings in the balance of the building by more than 10%, and 2) the total area of openings in a wall that receives positive external pressure exceeds 4 ft2 or 1% of the area of that wall, whichever is smaller, and also the percentage of openings in the balance of the building envelope does not exceed 20%).

Internal pressure coefficients, (***GCpi***), is determined from Table 26.11-1