Enclosure is classified in accordance with ASCE7-10 section 26.2, as **Open** since it is a building in which the area of the openings in each of the walls, receiving positive external pressure (***Ao***) exceeds 80% of the gross area of each such wall (***Ag***):

Internal pressure coefficients, (***GCpi***), is determined from Table 26.11-1