Using analytical procedure for components and cladding. Since h = ~h use Part 3 (for enclosed or partially enclosed building with h >60 ft). Design wind pressures are calculated as per ASCE7-10 Equation 30.6-1

Design wind pressure for components and cladding is: