Using Directional Procedure for buildings of all heights, design wind pressures for the MWFRS of the building is calculated as per ASCE7-10 Equation 27.4-1. Since in accordance with Table 26.11-1 internal pressure is applied to all surfaces, the net effect of internal pressure is zero. Therefore the term is omitted.

For windward side

For leeward side

Total net pressure