Using Directional Procedure for buildings of all heights, design wind pressures for the MWFRS of the building is calculated as per ASCE7-10 Equation 27.4-1

Design wind pressure for the MWFRS is: