The lateral-torsional buckling modification factor ***Cb***, for nonuniform moment diagrams (when both ends of the segment are braced) is determined as: