In order to calculate effective radius of gyration coefficient ***c*** is calculated as per Eq. (F2-8a)