Effective radius of gyration is calculated as per Eq. (F2-7)