Moment corresponding to plastic stress distribution (for calculation of weak-axis yielding limit state) is determined as per Eq. (F6-1)