Mapped MCER, 5% damped, spectral response acceleration parameter at a period of 1 s ***S1*** is obtained by interpolating USGS data used for ASCE7-10 Figure 22-2 for the location having Latitude ~Latitude, and Longitude ~Longitude.