Mapped MCER, 5% damped, spectral response acceleration parameter at short periods ***SS*** is obtained by interpolating USGS data used for ASCE7-10 Figure 22-1 for the location having Latitude ~Latitude, and Longitude ~Longitude.