Ground snow load, ***pg*** for the location having Latitude ~Latitude, and Longitude ~Longitude must be determined based on site-specific Case Studies, since site elevation ~Z ft exceeds elevation limit identified in ASCE7-10 figure 7-1 (~Max).