Ground snow load, ***pg*** is taken from NY State Building Code figure 1608.2 for the location having Latitude ~Latitude, and Longitude ~Longitude.

Since site elevation ~Z ft > 1,000 feet no ground snow load is increased from the mapped value by 2 psf for every 100 feet above 1,000 feet.