Ground snow load, ***pg*** is taken from NY State Building Code figure 1608.2 for the location having Latitude ~Latitude, and Longitude ~Longitude.

Since site elevation ~Z ft < 1,000 feet no ground snow load adjustment is required.